{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["waste management 1","waste management 2","waste management 3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"waste management 1","index":0,"n_rows":57,"n_cols":3,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[null,"Pareto Analysis: Waste ","Perte"]
[null,"causes des Pertes ","Perte"]
[null,"machin bidule",5000]
[null,"Huile hydraulique",4237]
[null,"Perte Transpalette ",1487]
[null,"TCA21",1184]
[null,"Perte Préparation ",875]
[null,"Boucle libre vide URA",801]
[null,"Echantillonneur",789]
[null,"Air stérile",785]
[null,"Défaut traitement",500]
[null,"Pulvérisation",489]
[null,"Nettoyage Intermédiare ",458]
[null,"Chambre aseptique",456]
[null,"Température armoire électrique",456]
[null,"Servomoteur",452]
[null,"Four",394]
[null,"Languette ouverture",375]
[null,"Perte Echantillon en cours de Production ",369]
[null,"Autre Perte Partie superieure ",320]
[null,"Hélix ",258]
[null,"Autre Perte DE",245]
[null,"Toboggan",242]
[null,"Changement du tank",238]
[null,"Autre Perte Logistique ",196]
[null,"Surcharge poste de sortie",189]
[null,"Débit eau soudure bas",178]
[null,"Roue à godets",147]
[null,"Dispatcheur  ",147]
[null,"Fin Bobine Patch",145]
[null,"Couronne de Formation ",142]
[null,"Changement de format",125]
[null,"Perte Retourneur Bobine ",123]
[null,"Système de nettoyage",123]
[null,"Raccord Film",117]
[null,"Laisser passer TLS",111]
[null,"Absence Opérateur",91]
[null,"Décors hors limites",85]
[null,"Non Respect du standard",81]
[null,"Stérilisateur",78]
[null,"Languette intérieure",74]
[null,"température d'eau de refroidissement",63]
[null,"Raccord Papier",60]
[null," Perte Chariot logistique ",50]
[null,"Peroxyde",48]
[null,"Surcharge moteur",47]
[null,"Rupture Papier URA",41]
[null,"Convoyeur",26]
[null,"Système lecture de niveau ",20]
[null,"correction Volume",17]
[null,"Reservoire de Peroxyde  ",16]
[null,"Echangeur de chaleur",14]
[null,"Fin Bobine Aluminium",12]
[null,"Batterie de chauffe",12]
[null," Nettoyage Complet",5]
[null,"Perte (Humidité)",5]
[null,"Autre Perte organisationnelProduction ",1]

{"sheet":"waste management 2","index":1,"n_rows":57,"n_cols":3,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[null,"Pareto Analysis: Waste ","Perte"]
[null,"causes des Pertes ","Perte"]
[null,"Truc muche",5000]
[null,"Huile hydraulique",4237]
[null,"Perte Transpalette ",1487]
[null,"TCA21",1184]
[null,"Perte Préparation ",875]
[null,"Boucle libre vide URA",801]
[null,"Echantillonneur",789]
[null,"Air stérile",785]
[null,"Défaut traitement",500]
[null,"Pulvérisation",489]
[null,"Nettoyage Intermédiare ",458]
[null,"Chambre aseptique",456]
[null,"Température armoire électrique",456]
[null,"Servomoteur",452]
[null,"Four",394]
[null,"Languette ouverture",375]
[null,"Perte Echantillon en cours de Production ",369]
[null,"Autre Perte Partie superieure ",320]
[null,"Hélix ",258]
[null,"Autre Perte DE",245]
[null,"Toboggan",242]
[null,"Changement du tank",238]
[null,"Autre Perte Logistique ",196]
[null,"Surcharge poste de sortie",189]
[null,"Débit eau soudure bas",178]
[null,"Roue à godets",147]
[null,"Dispatcheur  ",147]
[null,"Fin Bobine Patch",145]
[null,"Couronne de Formation ",142]
[null,"Changement de format",125]
[null,"Perte Retourneur Bobine ",123]
[null,"Système de nettoyage",123]
[null,"Raccord Film",117]
[null,"Laisser passer TLS",111]
[null,"Absence Opérateur",91]
[null,"Décors hors limites",85]
[null,"Non Respect du standard",81]
[null,"Stérilisateur",78]
[null,"Languette intérieure",74]
[null,"température d'eau de refroidissement",63]
[null,"Raccord Papier",60]
[null," Perte Chariot logistique ",50]
[null,"Peroxyde",48]
[null,"Surcharge moteur",47]
[null,"Rupture Papier URA",41]
[null,"Convoyeur",26]
[null,"Système lecture de niveau ",20]
[null,"correction Volume",17]
[null,"Reservoire de Peroxyde  ",16]
[null,"Echangeur de chaleur",14]
[null,"Fin Bobine Aluminium",12]
[null,"Batterie de chauffe",12]
[null," Nettoyage Complet",5]
[null,"Perte (Humidité)",5]
[null,"Autre Perte organisationnelProduction ",1]

{"sheet":"waste management 3","index":2,"n_rows":60,"n_cols":2,"rows_kept":60,"cut":false,"hidden":false,"merged":[]}
["causes des Pertes ","Perte"]
["Truc muche",5000]
["Huile hydraulique",4237]
["Perte Transpalette ",1487]
["TCA21",1184]
["Perte Préparation ",875]
["Boucle libre vide URA",801]
["Echantillonneur",789]
["Air stérile",785]
["Défaut traitement",500]
["Pulvérisation",489]
["Nettoyage Intermédiare ",458]
["Chambre aseptique",456]
["Température armoire électrique",456]
["Servomoteur",452]
["Four",394]
["Languette ouverture",375]
["Perte Echantillon en cours de Production ",369]
["Autre Perte Partie superieure ",320]
["Hélix ",258]
["Autre Perte DE",245]
["A",0]
["B",0]
["Toboggan",242]
["Changement du tank",238]
["Autre Perte Logistique ",196]
["D",0]
["Surcharge poste de sortie",189]
["Débit eau soudure bas",178]
["F",7000]
["Roue à godets",147]
["Dispatcheur  ",147]
["Fin Bobine Patch",145]
["Couronne de Formation ",142]
["Changement de format",125]
["Perte Retourneur Bobine ",123]
["Système de nettoyage",123]
["Raccord Film",117]
["Laisser passer TLS",111]
["Absence Opérateur",91]
["Décors hors limites",85]
["Non Respect du standard",81]
["Stérilisateur",78]
["Languette intérieure",74]
["température d'eau de refroidissement",63]
["Raccord Papier",60]
[" Perte Chariot logistique ",50]
["Peroxyde",48]
["Surcharge moteur",47]
["Rupture Papier URA",41]
["Convoyeur",26]
["Système lecture de niveau ",20]
["correction Volume",17]
["Reservoire de Peroxyde  ",16]
["Echangeur de chaleur",14]
["Fin Bobine Aluminium",12]
["Batterie de chauffe",12]
[" Nettoyage Complet",5]
["Perte (Humidité)",5]
["Autre Perte organisationnelProduction ",1]